# For more options and information see
# http://rpf.io/configtxt
# Some settings may impact device functionality. See link above for details

# HAOS - don't change it!
disable_splash=1
kernel=u-boot.bin

# uncomment for aarch64 bit support
#arm_64bit=1

# uncomment to enable primary UART console
#enable_uart=1

# uncomment if you get no picture on HDMI for a default "safe" mode
#hdmi_safe=1

# uncomment this if your display has a black border of unused pixels visible
# and your display can output without overscan
#disable_overscan=1

# uncomment the following to adjust overscan. Use positive numbers if console
# goes off screen, and negative if there is too much border
#overscan_left=16
#overscan_right=16
#overscan_top=16
#overscan_bottom=16

# uncomment to force a console size. By default it will be display's size minus
# overscan.
#framebuffer_width=1280
#framebuffer_height=720

# uncomment if hdmi display is not detected and composite is being output
#hdmi_force_hotplug=1

# uncomment to force a specific HDMI mode (this will force VGA)
#hdmi_group=1
#hdmi_mode=1

# uncomment to force a HDMI mode rather than DVI. This can make audio work in
# DMT (computer monitor) modes
#hdmi_drive=2

# uncomment to increase signal to HDMI, if you have interference, blanking, or
# no display
#config_hdmi_boost=4

# uncomment for composite PAL
#sdtv_mode=2

# Uncomment to disable continous SD-card poll (for USB SSD)
#dtparam=sd_poll_once=on

# Uncomment some or all of these to enable the optional hardware interfaces
#dtparam=i2c_arm=on
#dtparam=i2s=on
#dtparam=spi=on

# Uncomment this to enable the lirc-rpi module
#dtoverlay=lirc-rpi

# Uncomment this to enable GPIO support for RPI-RF-MOD/HM-MOD-RPI-PCB
#enable_uart=1
#dtparam=i2c_arm=on
#dtoverlay=miniuart-bt
#dtoverlay=rpi-rf-mod

# Additional overlays and parameters are documented /boot/overlays/README

# Enable audio (loads snd_bcm2835)
dtparam=audio=on

[all]
#dtoverlay=vc4-fkms-v3d
#max_framebuffers=2
