BR2_aarch64=y
BR2_cortex_a53=y
BR2_ARM_FPU_VFPV4=y

# Linux headers same as kernel, a 4.14 series
BR2_PACKAGE_HOST_LINUX_HEADERS_CUSTOM_4_14=y

# Firmware
BR2_TARGET_ARM_TRUSTED_FIRMWARE=y
BR2_TARGET_ARM_TRUSTED_FIRMWARE_CUSTOM_GIT=y
BR2_TARGET_ARM_TRUSTED_FIRMWARE_CUSTOM_REPO_URL="https://github.com/apritzel/arm-trusted-firmware.git"
BR2_TARGET_ARM_TRUSTED_FIRMWARE_PLATFORM="sun50iw1p1"
BR2_TARGET_ARM_TRUSTED_FIRMWARE_CUSTOM_REPO_VERSION="aa75c8da415158a94b82a430b2b40000778e851f"
BR2_TARGET_ARM_TRUSTED_FIRMWARE_BL31=y

# Bootloader
BR2_TARGET_UBOOT=y
BR2_TARGET_UBOOT_BUILD_SYSTEM_KCONFIG=y
BR2_TARGET_UBOOT_CUSTOM_VERSION=y
BR2_TARGET_UBOOT_CUSTOM_VERSION_VALUE="2017.11"
BR2_TARGET_UBOOT_BOARD_DEFCONFIG="orangepi_prime"
BR2_TARGET_UBOOT_NEEDS_DTC=y
BR2_TARGET_UBOOT_NEEDS_ATF_BL31=y
BR2_TARGET_UBOOT_FORMAT_CUSTOM=y
BR2_TARGET_UBOOT_FORMAT_CUSTOM_NAME="u-boot.itb"
BR2_TARGET_UBOOT_SPL=y
BR2_TARGET_UBOOT_SPL_NAME="spl/sunxi-spl.bin"
BR2_TARGET_UBOOT_BOOT_SCRIPT=y
BR2_TARGET_UBOOT_BOOT_SCRIPT_SOURCE="board/orangepi/orangepi-prime/boot.cmd"

# Kernel
BR2_LINUX_KERNEL=y
BR2_LINUX_KERNEL_CUSTOM_VERSION=y
BR2_LINUX_KERNEL_CUSTOM_VERSION_VALUE="4.14"
BR2_LINUX_KERNEL_USE_ARCH_DEFAULT_CONFIG=y
BR2_LINUX_KERNEL_DTS_SUPPORT=y
BR2_LINUX_KERNEL_INTREE_DTS_NAME="allwinner/sun50i-h5-orangepi-prime"

# Filesystem
BR2_TARGET_GENERIC_ISSUE="Welcome to Orangepi Prime"
BR2_TARGET_ROOTFS_EXT2=y
BR2_TARGET_ROOTFS_EXT2_4=y
BR2_PACKAGE_HOST_DOSFSTOOLS=y
BR2_PACKAGE_HOST_GENIMAGE=y
BR2_PACKAGE_HOST_MTOOLS=y
BR2_ROOTFS_POST_IMAGE_SCRIPT="support/scripts/genimage.sh"
BR2_ROOTFS_POST_SCRIPT_ARGS="-c board/orangepi/orangepi-prime/genimage.cfg"
