# Architecture
BR2_arm=y
BR2_arm926t=y

# Toolchain
BR2_PACKAGE_HOST_ELF2FLT=y
# BR2_USE_MMU is not set

# Patches
BR2_GLOBAL_PATCH_DIR="board/qemu/arm-versatile/patches"

# Busybox with hush
BR2_PACKAGE_BUSYBOX_CONFIG="package/busybox/busybox-minimal.config"

# System
BR2_SYSTEM_DHCP="eth0"
BR2_TARGET_GENERIC_GETTY_PORT="ttyAMA0"

# Filesystem
# BR2_TARGET_ROOTFS_EXT2 is not set
# BR2_TARGET_ROOTFS_TAR is not set
BR2_TARGET_ROOTFS_INITRAMFS=y

# Linux headers same as kernel, a 4.4 series
BR2_PACKAGE_HOST_LINUX_HEADERS_CUSTOM_4_4=y

# Kernel
BR2_LINUX_KERNEL=y
BR2_LINUX_KERNEL_CUSTOM_VERSION=y
BR2_LINUX_KERNEL_CUSTOM_VERSION_VALUE="4.4.70"
BR2_LINUX_KERNEL_USE_CUSTOM_CONFIG=y
BR2_LINUX_KERNEL_CUSTOM_CONFIG_FILE="board/qemu/arm-versatile/linux-4.4-nommu.config"
